{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["VACA_Sheet","Sheet2"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"VACA_Sheet","index":0,"n_rows":44,"n_cols":37,"rows_kept":44,"cut":false,"hidden":false,"merged":[[38,0,38,5],[0,3,0,5],[11,0,11,5],[25,0,25,5],[5,1,5,2],[6,1,6,2],[5,4,5,5],[6,4,6,5]]}
[null,null,null,"Valve / Actuator / Controls Application Sheet"]
[]
[]
["8000 Market Street, Suite 240, Houston, TX 77029   Phn: 713.747.1500   Email: info@avctexas.com   Web: avctexas.com"]
[]
["Company:",null,null,"Telephone:"]
["Contact:",null,null,"Email:"]
[]
[]
["Item #:",1,2,3,4,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes / No","Valve Types","End Conns","Rating",null,"Actuator Types","Power Types","Enclosure Rating","D/A or S/R","Elect Act Options","Modulating / On/off"]
["Quantity:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Ball Vlv - Full Port","Flanged - RF",125,null,"Electric","Enter Voltage Here","Explosion Proof","Double Acting","Aux. Switches","Modulating"]
["Valve Data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","Ball Vlv - Reduced Port","Flanged - RTJ",150,null,"Electro-Hydraulic","Enter Voltage Here","Weather Proof","Fail in Place","Brake","On / Off"]
["Valve Type:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bfly Vlv  Resil. Seated","Threaded",300,null,"Gear Operator - Declutch.","Manual",null,"S/R Fail Close (CW)"]
["Size (Inch):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bfly Vlv  Hi-Perf","Lug",600,null,"Gear Operator - Non-Declutch.","Manual",null,"S/R Fail Open (CCW)"]
["End Conn:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gate Vlv - OSY","Wafer",900,null,"Hydraulic","Enter Min. Supply Press. Here"]
["Rating:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gate Vlv - NRS","Welded - Buttweld",1500,null,"Lever","Manual"]
["Body Mat'l:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Globe Vlv","Welded - Weldneck",2500,null,"Pneumatic","Enter Min. Supply Press. Here"]
["Trim / Disc Mat'l:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damper"]
["Seat Mat'l:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other*: See column bottom."]
["Max DP (in psi):"]
["Rotary Valve Torque:\nBreak / Run / Reseat (In-Lb)"]
["Linear Valve Thrust:\nMax Thrust (Lbs)"]
["Media:"]
["*Other \"Valve\" Type:"]
[]
["Actuator Data"]
["Actuator Type:"]
["Power:",{"$f":"IF(B27=\"\",\"\",LOOKUP(B27,$AF$11:$AF$17,$AG$11:$AG$17))","v":""},{"$f":"IF(C27=\"\",\"\",LOOKUP(C27,$AF$11:$AF$17,$AG$11:$AG$17))","v":""},{"$f":"IF(D27=\"\",\"\",LOOKUP(D27,$AF$11:$AF$17,$AG$11:$AG$17))","v":""},{"$f":"IF(E27=\"\",\"\",LOOKUP(E27,$AF$11:$AF$17,$AG$11:$AG$17))","v":""},{"$f":"IF(F27=\"\",\"\",LOOKUP(F27,$AF$11:$AF$17,$AG$11:$AG$17))","v":""}]
["D/A or S/R, etc.:"]
["Elect. Encl. Rating:"]
["Modulating or On/Off:"]
["Manual Override:"]
["Brake (Elect. Act):"]
["Aux. Sw's (Elect. Act.):"]
["Enter Other Options:"]
["Special Notes:"]
[null,{"$f":"IF(MID(B13,1,4)<>\"Bfly\",\"\",IF(MID(B27,1,4)=\"Elec\",IF(B33<>\"YES\",\"Bfly Vlv REQUIRES Brake!\",\"\"),\"\"))","v":""},{"$f":"IF(MID(C13,1,4)<>\"Bfly\",\"\",IF(MID(C27,1,4)=\"Elec\",IF(C33<>\"YES\",\"Bfly Vlv REQUIRES Brake!\",\"\"),\"\"))","v":""},{"$f":"IF(MID(D13,1,4)<>\"Bfly\",\"\",IF(MID(D27,1,4)=\"Elec\",IF(D33<>\"YES\",\"Bfly Vlv REQUIRES Brake!\",\"\"),\"\"))","v":""},{"$f":"IF(MID(E13,1,4)<>\"Bfly\",\"\",IF(MID(E27,1,4)=\"Elec\",IF(E33<>\"YES\",\"Bfly Vlv REQUIRES Brake!\",\"\"),\"\"))","v":""},{"$f":"IF(MID(F13,1,4)<>\"Bfly\",\"\",IF(MID(F27,1,4)=\"Elec\",IF(F33<>\"YES\",\"Bfly Vlv REQUIRES Brake!\",\"\"),\"\"))","v":""}]
[]
["Controls / Options"]
["Limit Switches:\n"]
["Solenoid Valve:\n(Include Voltage, etc.)"]
["Position Indicator:\n(With or Without L.S.)"]
["Positioner:\n(Describe. I/P, E/P, etc.)"]
["Other (Specify):\n"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}